00.010.020.03

Rrs(412)0.010.1110100In situ Chl a (mg.m-3)05101520

Rrs(412)/Rrs(555)0.010.1110100In situ Chl a (mg.m-3)Figure 1. Example of quality control procedure used to identify outliers in the SeaBAM data set. Upper panel: Scatter plotof Rrs(412) vs in situ [Chl a]. Problems with stations marked with diamonds, triangles and circles were identified as relatedto calibration issues or errors in data processing. Lower panel: Scatter plot of Rrs(412)/Rrs(555) vs in situ [Chl a] for thesame stations (see text).